Text consolidated by Valsts valodas centrs (State Language Centre) with amending regulations of:
19 December 2024 [shall come into force on 29 December 2024].
If a whole or part of a paragraph has been amended, the date of the amending regulation appears in square brackets at the end of the paragraph. If a whole paragraph or sub-paragraph has been deleted, the date of the deletion appears in square brackets beside the deleted paragraph or sub-paragraph.


Decision No. 1/24 of the Board of the Public Utilities Commission

Adopted 15 September 2022


Regulations Regarding Unbundled Access to the Subscriber Line


Issued pursuant to
Section 80, Paragraph three and Section 83, Paragraph one, Clause 2 of the Electronic Communications Law

[bookmark: n1][bookmark: n-1135271]I. General Provisions

[bookmark: p1][bookmark: p-1396082]1. The regulations prescribe:
1.1. the technical and operational conditions of an electronic communications network for an electronic communications merchant with a significant market power who has a specific access obligation to ensure unbundled access to a subscriber line (hereinafter – the owner) for the following types of access:
1.1.1. full unbundled access to the subscriber line – an electronic communications service provided by the lessee to the end-user, using the subscriber line over its whole length;
1.1.2. [19 December 2024];
1.1.3. full unbundled access to the part of the subscriber line, including to the terminating segment – an electronic communications service provided by the lessee to the end-user, using the segment of the subscriber line from the distribution point to the termination point unless the owner and the lessee have agreed otherwise;
1.1.4. [19 December 2024];
1.2. the technical information to be included in a reference offer for unbundled access to the subscriber line and the level of detail thereof.
[19 December 2024]
[bookmark: p2][bookmark: p-1396084]
2. The following terms are used in the regulations:
2.1. unbundled access to the subscriber line (hereinafter – the unbundled access) – an access service provided by the owner to another electronic communications merchant for the provision of the electronic communications service, using the subscriber line or part thereof fully or jointly;
2.2. backhaul – the following service established between the unbundled access point and the electronic communications network facility of the lessee:
2.2.1. Ethernet backhaul – a connection established at the Ethernet OSI Layer 2;
2.2.2. access to cable ducts or poles;
2.3.3. lease of dark fibre;
2.3. lessee – an electronic communications merchant who has entered into a contract for the unbundled access with the owner;
2.4. central office – a place where the access network and the core network interconnect;
2.5. unbundled access point – a physical point collocated at the central office of the owner or another place over the electronic communications network, if technically possible, at which the owner provides the lessee with unbundled access to the subscriber line to provide the electronic communications services to the end-user over the subscriber line of the owner;
2.6. backhaul access point – a physical point collocated at the central office of the owner or another place over the electronic communications network, if technically possible, at which the owner provides the lessee with the backhaul;
2.7. Ethernet backhaul access point – an interface of the electronic communications network facility of the owner at which the owner provides the lessee with the Ethernet backhaul;
2.8. applicant – an electronic communications merchant who wishes to obtain unbundled access;
2.9. distribution point – a cable distribution device for the public electronic communications network which is intended for the distribution of metallic or optical fibre cables. The distribution point is a cable distribution cabinet, distribution box, small distribution box, or cable closure;
2.10. [19 December 2024];
2.11. dark fibre – an optical fibre in an installed or built cable line which is not active, i.e. its both ends are not connected to operating optoelectronic devices;
2.12. virtual unbundled local access (VULA) – an active access product which is a connection established at the Ethernet OSI Layer 2 between the connection point of the subscriber line of the owner and the unbundled access point and which is physically collocated at the central office of the owner or another place over the electronic communications network.
[bookmark: p3][bookmark: p-1396087]
3. The following abbreviations are used in the regulations:
3.1. Ethernet P2P – Ethernet Point to Point Technology;
3.2. FTTB (Fibre to the Building) – ensuring of optical fibre cables to the building;
3.3. FTTH (Fibre to the Home) – ensuring of optical fibre cables to the premises of an end-user;
3.4. FTTN (Fibre to the Node) – ensuring of optical fibre cables to the distribution cabinet;
3.5. Gbit/s – gigabits per second;
3.6. [19 December 2024];
3.7. IGMP – Internet Group Multicast Protocol;
3.8. ITU-T – International Telecommunications Union, Telecommunication Standardization Sector;
3.9. MDF (Main Distribution Frame) – shielded twisted pair cable cross;
3.10. NTU – Network Termination Unit;
3.11. ODF (Optical Fibre Distribution Frame) – optical fibre cable cross;
3.12. OSI – Open Systems Interconnection;
3.12.1 PON – passive optical network;
3.13. [19 December 2024];
3.14. TP – termination point;
3.15. P2P (Point to Point) – access network point-to-point architecture;
3.16. RJ (Registered Jack) – a standardised physical interface of an electronic communications network;
3.17. [19 December 2024];
3.18. [19 December 2024];
3.19. VLAN – Virtual Local Area Network;
3.20. VULA – Virtual Unbundled Local Access;
3.21. [19 December 2024].
[19 December 2024]
[bookmark: p4][bookmark: p-1396088]
4. Technological solutions for unbundling refer to the subscriber line established in accordance with the general organisation chart of the access network indicated in Annex 1 to these regulations and the access network architecture of optical fibre cables indicated in Annex 2 to these regulations.
[19 December 2024]
[bookmark: p5][bookmark: p-1135290]
5. The owner shall include in the reference offer for unbundled access to the subscriber line at least the following technological solutions used over its access network and indicated in Annex 3 to these regulations:
5.1. access network architecture;
5.2. access network technology;
5.3. type of unbundled access;
5.4. unbundling technology;
5.5. place for the implementation of unbundled access.
[bookmark: p6][bookmark: p-1396089]
6. The owner shall use at least the following unbundling technologies for the implementation of unbundled access:
6.1. physical switching:
6.1.1. the physical switching of the terminating segment of the FTTB subscriber line is the mechanical switching of the shielded twisted pairs at the distribution point using a terminator, a connector module, or a connector; it also includes the switching of the pair not in use of the terminating segment of the FTTB subscriber line at the subscriber line distribution point;
6.1.2. physical switching over the optical fibre cable subscriber line is mechanical switching of the optical fibres at the central office or distribution point by using the optical plug and coupler or fibre connection; it also includes switching of the dark fibre over the access network at the unbundling place necessary for the applicant – at the ODF of the central office, distribution point of the subscriber line, or termination point, and also connection for the drawable fibre cable fibre;
6.2. [19 December 2024];
6.3. VULA.
[19 December 2024]
[bookmark: p7][bookmark: p-1396090]
7. [19 December 2024]
[bookmark: p8][bookmark: p-1135299]
8. In the reference offer for unbundled access to the subscriber line, the owner shall include the technical requirements for the shielded optical fibre cable subscriber line and dark fibre which are applicable to unbundled access, covering at least the following conditions:
8.1. the requirements for the optical fibre, indicating the European standard and ITU-T recommendation to which the optical fibre conforms;
8.2. attenuation in optical fibre (dB/km) at wavelengths of electromagnetic waves of 1310 nm, 490 nm, and 1550 nm if the applicant intends to use a facility operating at other wavelengths of electromagnetic waves, the owner shall, upon request of the applicant, within five working days, provide the applicant individually with attenuation in optical fibre (dB/km) at the requested wavelengths of electromagnetic waves;
8.3. the requirements for the optical plug and coupler;
8.4. the requirements for lightning and over-voltage protection equipment and the procedures for the installation thereof.
[bookmark: p9][bookmark: p-1396092]
9. For unbundled access to FTTH P2P or PON, FTTB access network architectures and technology, except for terminating segment, the owner shall provide, upon request of the lessee, the backhaul for Ethernet, lease of dark fibre, or access cable ducts. In case of other access network technologies, the owner shall provide the backhaul upon agreement with the lessee.
[19 December 2024]
[bookmark: p10][bookmark: p-1396093]
10. For unbundled access to FTTH P2P or PON, FTTB access network architectures and technology, except for terminating segment, the following additional requirements shall be complied with by the owner when providing the Ethernet backhaul:
10.1. an access point shall be established for the Ethernet backhaul as the optical fibre connector of the Ethernet OSI Layer 2 distribution frame where the following maximum download and upload data transmission speed (hereinafter – the transmission speed) shall be ensured: 1*n Gbit/s where n is a natural figure which is greater than 0 and the value of which is determined upon agreement between the lessee and the owner;
10.2. it shall be ensured at the access point for the Ethernet backhaul that the lessee has a possibility to control the transmission speed of the service provided to the end-users;
10.3. the quality requirements in accordance with Paragraph 20 of these regulations.
[19 December 2024]
[bookmark: p11][bookmark: p-1135316]
11. The owner shall ensure the guaranteed transmission speed for the Ethernet backhaul which is not less than 80 % of the connection speed.
[bookmark: p12][bookmark: p-1135318]
12. The owner and the lessee shall agree upon the technical requirements for the subscriber line, and also upon the wavelength of electromagnetic wave to be used, the range of frequency spectrum, the level of signal transmission, the line code to be used in the signal transmission, or any other conditions, taking into account the technical requirements for the facility to be used if other or additional parameters are applicable to the connection of the facility used by the lessee, and also if it is indented to use such technology or technical solution for unbundled access which does not correspond to the technical parameters ensured for the subscriber line.
[bookmark: p13][bookmark: p-1135320]
13. In the reference offer for unbundled access to the subscriber line, the owner shall include the technical requirements for electrical interfaces for virtual unbundling at the following points of the electronic communications network:
13.1. termination point;
13.2. unbundled access point;
13.3. access point for the Ethernet backhaul.
[bookmark: p14][bookmark: p-1396094]
14. The owner shall ensure the applicant with the following interfaces for NTUs at the network termination point for unbundled access:
14.1. without an active NTU. At the termination point of shielded twisted pair cables of the terminating segment of the FTTB subscriber line, a physical NTU is an outlet with an appropriate RJ type socket. At the termination point of optical fibre cables, a physical NTU is an optical plug;
14.2. with an active NTU. If chosen by the applicant, the owner shall ensure an active NTU at the termination point.
[19 December 2024]
[bookmark: p15][bookmark: p-1135328]
15. In the reference offer for unbundled access to the subscriber line, the owner shall include a list of compatible active NTUs, indicating the manufacturer and the name of facility assigned by the manufacturer, and shall update the list once a year. If the owner ensures an active NTU, then the brand of the owner or other information identifying the owner shall not be indicated on the NTU.
[bookmark: p16][bookmark: p-1135329]
16. In the case of virtual unbundling, the owner shall ensure an Ethernet access point for unbundled access with the following physical interfaces and the maximum transmission speeds, offering the lessee a possibility to control the transmission speed of the service provided to the end-user:
16.1. an RJ type socket in which the following transmission speed is ensured: 0.1*n Gbit/s where n is a natural figure which is greater than 0 and the value of which is determined upon agreement between the lessee and the owner;
16.2. an optical fibre connector in which the following transmission speed is ensured: 1*n Gbit/s where n is a natural figure which is greater than 0 and the value of which is determined upon agreement between the lessee and the owner;
16.3. the quality requirements in accordance with Paragraph 20 of these regulations.
[bookmark: p17][bookmark: p-1135330]
17. The owner shall ensure the guaranteed transmission speed at the Ethernet access point for unbundled access which is not less than 80 % of the connection speed.
[bookmark: p18][bookmark: p-1135331]
18. The owner shall ensure the access point for the Ethernet backhaul for the unbundled access voice service, Internet access service, and television programme distribution service with a contention ratio in accordance with the agreement between the lessee and the owner.
[bookmark: p19][bookmark: p-1135332]
19. In the case of virtual unbundling, the owner shall include in the reference offer for unbundled access to the subscriber line at least the following service categories for the Ethernet backhaul for download and upload:
19.1. voice telephony service category;
19.2. Internet access service category;
19.3. television programme distribution service category.
[bookmark: p20][bookmark: p-1396095]
20. In the case of virtual unbundling, the owner shall include in the reference offer for unbundled access to the subscriber line at least the following quality requirements for the Ethernet backhaul for each service category which shall not be lower than those for the service provided by the owner in retail:
20.1. traffic transmission priorities in the network of the owner, indicating the methods for setting priorities which have been specified in the priority frame and offering a possibility for the lessee to determine the priority for the traffic;
20.2. one-way frame delay;
20.3. inter-frame delay variation;
20.4. frame loss;
20.5. availability.
[19 December 2024]
[bookmark: p21][bookmark: p-1135335]
21. In the case of virtual unbundling, the owner shall, upon request of the lessee, provide multicast in the following manner:
21.1. by using the IGMP protocol with replication of television flow for the end-user in the owner’s central office facilities of the local level;
21.2. by assigning the lessee a separate VLAN for the television programme distributions service.
[bookmark: p22][bookmark: p-1135337]
22. In the case of virtual unbundling and if requested by the lessee, the owner shall provide each end-user of the lessee with its own VLAN when providing the voice service or Internet access service. In the case of virtual unbundling, the lessee shall determine security requirements in its electronic communications network.
[bookmark: p23][bookmark: p-1135339]
23. In the case of virtual unbundling and Ethernet backhaul, the owner shall ensure the lessee with a possibility to apply security measures.
[bookmark: p24][bookmark: p-1135340]
24. In the case of virtual unbundling and Ethernet backhaul, the owner shall provide the lessee with a possibility to identify its end-users on the level of central office facilities or VLAN.
[bookmark: p25][bookmark: p-1135341]
25. Decision No. 1/11 of the Public Utilities Commission of 18 June 2014, Regulations Regarding Unbundled Access to the Subscriber Line or Part Thereof (Latvijas Vēstnesis, 2014, No. 120; 2018, No. 199), is repealed.
[bookmark: p26][bookmark: p-1135342]
26. The regulations shall come into force on 1 October 2022.


Chair of the Board of the Public Utilities Commission	A. Ozola
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[bookmark: 1135348][bookmark: n-1135348]General Organisation Chart of the Access Network
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[bookmark: 1135356][bookmark: n-1135356]Access Network Architecture of Shielded Twisted Pairs and Optical Fibre Cables


1. Division of access network architectures
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2. Access network point-to-point architecture
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3. Access network point-to-multipoint architecture and three basic options of the placement of a point-to-multipoint facility
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4. Access network architecture of optical fibre cables – depending on the termination point of optical fibre cable over the subscriber line
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Technological Solutions for Unbundled Access


1. [19 December 2024]

2. Unbundled access in the optical fibre cable access network (FTTH)
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3. Unbundled access in the optical fibre cable access network (FTTB)
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4. [19 December 2024]
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